XSynchronization Extention Protocol

XConsortium Standard

Tim Glauert, Olivetti Research/MultiWorks

Dave Carver

Digital EquipmentCorporation, MIT/Project Athena

Jim Gettys

Digital EquipmentCorporation, Cambridge Research Laboratory

David Wiggins

XConsortium, Inc.

XSynchronization Extention Protocol: XConsortium Standard

by Tim Glauert

Dave Carver

Digital EquipmentCorporation, MIT/Project Athena

Jim Gettys

Digital EquipmentCorporation, Cambridge Research Laboratory

David Wiggins

X Consortium, Inc.

X Version 11, Release 6.6.84

Version 3.0

Copyright © 1991 Olivetti Research Limited, Cambridge England and Digital Equipment Corporation, Maynard,

Massachusetts

Copyright © 1991 X Consortium

Permission to use, copy, modify, and distribute this documentation for any purpose and without fee is hereby granted, provided that the above copyright notice appear in all copies. Olivetti, Digital, MIT, and the X Consortium make no representations about the suitability for any purpose of the information in this document. This documentation is provided as is without express or implied warranty.

Permission is hereby granted, free of charge, to any person obtaining a copy of this software and associated documentation files (the "Software"), to deal in the Software without restriction, including without limitation the rights to use, copy, modify, merge, publish, distribute, sublicense, and/ or sell copies of the Software, and to permit persons to whom the Software is furnished to do so, subject to the following conditions:

The above copyright notice and this permission notice shall be included in all copies or substantial portions of the Software.

THE SOFTWARE IS PROVIDED “AS IS”, WITHOUT WARRANTY OF ANY KIND, EXPRESS OR IMPLIED, INCLUDING BUT NOT

LIMITED TO THE WARRANTIES OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND NONINFRINGEMENT.

IN NO EVENT SHALL THE X CONSORTIUM BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY, WHETHER IN AN

ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE

USE OR OTHER DEALINGS IN THE SOFTWARE.

Except as contained in this notice, the name of the X Consortium shall not be used in advertising or otherwise to promote the sale, use or other dealings in this Software without prior written authorization from the X Consortium.

iii Table of Contents

1. Synchronization Protocol .................................................................................................. 1

Description ................................................................................................................ 1

Types ....................................................................................................................... 1

Errors ....................................................................................................................... 3

Requests ................................................................................................................... 3

Events ...................................................................................................................... 8

2. Encoding ..................................................................................................................... 10

Encoding New Types ................................................................................................ 10

Encoding Errors ........................................................................................................ 10

Encoding Requests .................................................................................................... 11

Encoding Events ....................................................................................................... 14

1 Chapter 1. Synchronization Protocol

The core X protocol makes no guarantees about the relative order of execution of requests for different clients. This means that any synchronization between clients must be done at the client level in an operating system-dependent and network-dependent manner. Even if there was an accepted standard for such synchronization, the use of a network introduces unpredictable delays between the synchronization of the clients and the delivery of the resulting requests to the X server.

The core X protocol also makes no guarantees about the time at which requests are executed, which means that all clients with real-time constraints must implement their timing on the host computer. Any such timings are subject to error introduced by delays within the operating system and network and are inefficient because of the need for round-trip requests that keep the client and server synchronized.

The synchronization extension provides primitives that allow synchronization between clients to take place entirely within the X server. This removes any error introduced by the network and makes it possible to synchronize clients on different hosts running different operating systems. This is important for multimedia applications, where audio, video, and graphics data streams are being synchronized. The extension also provides internal timers within the X server to which client requests can be synchronized. This allows simple animation applications to be implemented without any round-trip requests and makes best use of buffering within the client, network, and server.

Description

The mechanism used by this extension for synchronization within the X server is to block the processing of requests from a client until a specific synchronization condition occurs. When the condition occurs, the client is released and processing of requests continues. Multiple clients may block on the same condition to give inter-client synchronization. Alternatively, a single client may block on a condition such as an animation frame marker.

The extension adds Counter and Alarm to the set of resources managed by the server. A counter has a 64-bit integer value that may be increased or decreased by client requests or by the server internally. A client can block by sending an Await request that waits until one of a set of synchronization conditions, called TRIGGERs, becomes TRUE.

The CreateCounter request allows a client to create a Counter that can be changed by explicit

SetCounterandChangeCounterrequests.Thesecanbeusedtoimplementsynchronizationbetween different clients.

There are some counters, calledSystem Counters,thatarechangedbytheserverinternallyratherthan by client requests. The effect of any change to a system counter is not visible until the server has finished processing the current request. In other words, system counters are apparently updated in the gaps between the execution of requests rather than during the actual execution of a request. The extension provides a system counter that advances with the server time as defined by the core protocol, and it may also provide counters that advance with the real-world time or that change each time the CRT screen is refreshed. Other extensions may provide their own extension-specific system counters.

The extension provides an Alarm mechanism that allows clients to receive an event on a regular basis when a particular counter is changed.

Types

Please refer to the X11 Protocol specification as this document uses syntactic conventions established there and references types defined there.

Synchronization Protocol 2 The following new types are used by the extension.

INT64: 64-bit signed integer

COUNTER: XID

VALUETYPE: {Absolute,Relative};

TESTTYPE: {PositiveTransition,NegativeTransition,

                        PositiveComparison,NegativeComparison}

TRIGGER: [

                        counter:COUNTER,

                        value-type:VALUETYPE,

                        wait-value:INT64,

                        test-type:TESTTYPE

                       ]

WAITCONDITION: [

                        trigger:TRIGGER,

                        event-threshold:INT64

                       ]

SYSTEMCOUNTER: [

                        name:STRING8,

                        counter:COUNTER,

                        resolution:INT64

                       ]

ALARM: XID

ALARMSTATE: {Active,Inactive,Destroyed}

The COUNTER type defines the client-side handle on a server Counter. The value of a counter is an

INT64.

The TRIGGER type defines a test on a counter that is either TRUE or FALSE. The value of the test is determined by the combination of a test value, the value of the counter, and the specified test-type.

The test value for a trigger is calculated using the value-type and wait-value fields when the trigger is initialized. If the value-type field is not one of the named VALUETYPE constants, the request that initialized the trigger will return a Value error. If the value-type field is Absolute, the test value is given by the wait-value field. If the value-type field is Relative, the test value is obtained by adding the wait-value field to the value of the counter. If the resulting test value would lie outside the range for an INT64, the request that initialized the trigger will return a Value error. If counter is None and the value-type is Relative, the request that initialized the trigger will return a Match error. If counter is not None and does not name a valid counter, a Counter error is generated.

If the test-type is PositiveTransition, the trigger is initialized to FALSE, and it will become TRUE when the counter changes from a value less than the test value to a value greater than or equal to the test value. If the test-type is NegativeTransition, the trigger is initialize to FALSE, and it will become

TRUE when the counter changes from a value greater than the test value to a value less than or equal to the test value. If the test-type is PositiveComparison, the trigger is TRUE if the counter is greater than or equal to the test value and FALSE otherwise. If the test-type is NegativeComparison, the trigger is TRUE if the counter is less than or equal to the test value and FALSE otherwise. If the test-type is not one of the named TESTTYPE constants, the request that initialized the trigger will return a Value error.

A trigger with a counter value of None and a valid test-type is always TRUE.

The WAITCONDITION type is simply a trigger with an associated event-threshold. The event threshold is used by theAwaitrequesttodecidewhetherornottogenerateaneventtotheclientafterthetriggerhas become TRUE. By setting the event-threshold to an appropriate value, it is possible to detect the situation where an Await request was processed after the TRIGGER became TRUE, which usually indicates that the server is not processing requests as fast as the client expects.

Synchronization Protocol 3 The SYSTEMCOUNTER type provides the client with information about a SystemCounter. The name field is the textual name of the counter that identifies the counter to the client. The counter field is the client-side handle that should be used in requests that require a counter. The resolution field gives the approximate step size of the system counter. This is a hint to the client that the extension may not be able to resolve two wait conditions with test values that differ by less than this step size. A microsecond clock, for example, may advance in steps of 64 microseconds, so a counter based on this clock would have a resolution of 64.

The only system counter that is guaranteed to be present is called SERVERTIME, which counts milliseconds from some arbitrary starting point. The least significant 32 bits of this counter track the value of Time used by the server in Events and Requests. Other system counters may be provided by different implementations of the extension. The X Consortium will maintain a registry of system counter names to avoid collisions in the name space.

An ALARM is the client-side handle on an Alarm resource.

Errors

Counter This error is generated if the value for a COUNTER argument in a request does not name a defined COUNTER.

Alarm This error is generated if the value for an ALARM argument in a request does not name a defined ALARM.

Requests

Initialize version-major,version-minor: CARD8

=>
version-major,version-minor: CARD8

This request must be executed before any other requests for this extension. If a client violates this rule, the results of all SYNC requests that it issues are undefined. The request takes the version number of the extension that the client wishes to use and returns the actual version number being implemented by the extension for this client. The extension may return different version numbers to a client depending of the version number supplied by that client. This request should be executed only once for each client connection.

Given two different versions of the SYNC protocol, v1 and v2, v1 is compatible with v2 if and only if v1.version_major = v2.version_major and v1.version_minor

<= v2.version_minor. Compatible means that the functionality is fully supported in an identical fashion in the two versions.

This document describes major version 3, minor version 0 of the SYNC protocol.

ListSystemCounters

=>
system-counters: LISTofSYSTEMCOUNTER

Synchronization Protocol

4 Errors: Alloc

This request returns a list of all the system counters that are available at the time the request is executed, which includes the system counters that are maintained by other extensions.

The list returned by this request may change as counters are created and destroyed by other extensions.

CreateCounter id: COUNTER
initial-value: INT64

Errors: IDChoice,Alloc

This request creates a counter and assigns the specified id to it. The counter value is initialized to the specified initialvalue and there are no clients waiting on the counter.

DestroyCounter counter: COUNTER

Errors: Counter,Access

This request destroys the given counter and sets the counter fields for all triggers that specify this counter to None.

All clients waiting on the counter are released and a

CounterNotify event with the destroyed field set to

TRUE is sent to each waiting client, regardless of the event-threshold. All alarms specifying the counter become

Inactive and an AlarmNotify event with a state field of Inactive is generated. A counter is destroyed automatically when the connection to the creating client is closed down if the close-down mode is Destroy. AnAccess error is generated if counter is a system counter. ACounter error is generated if counter does not name a valid counter.

QueryCounter counter: COUNTER

=>
value: INT64

Errors: Counter

This request returns the current value of the given counter or a generates Counter error if counter does not name a valid counter.

Await wait-list: LISTofWAITCONDITION

Errors: Counter,Alloc,Value

When this request is executed, the triggers in the wait-list are initialized using the wait-value and value-type fields, as described in the definition of TRIGGER above. The processing of further requests for the client is blocked until one or more of the triggers becomes TRUE. This may happen immediately, as a result of the initialization, or at some later time, as a result of a subsequent SetCounter,

ChangeCounter or DestroyCounter request.

Synchronization Protocol

5 A Value error is generated if wait-list is empty.

When the client becomes unblocked, each trigger is checked to determine whether a CounterNotify event should be generated. The difference between the counter and the test value is calculated by subtracting the test value from the value of the counter. If the test-type is PositiveTransition or PositiveComparison, a CounterNotify event is generated if the difference is at least eventthreshold. If the test-type is NegativeTransition or

NegativeComparison, a CounterNotify event is generated if the difference is at most event-threshold. If the difference lies outside the range for an INT64, an event is not generated.

This threshold check is made for each trigger in the list and a CounterNotify event is generated for every trigger for which the check succeeds. The check forCounterNotify events is performed even if one of the triggers is TRUE when the request is first executed. Note that a CounterNotify event may be generated for a trigger that is FALSE if there are multiple triggers in the request. A CounterNotify event with the destroyed flag set to TRUE is always generated if the counter for one of the triggers is destroyed.

ChangeCounter counter: COUNTER
amount: INT64

Errors: Counter,Access,Value

This request changes the given counter by adding amount to the current counter value. If the change to this counter satisfies a trigger for which a client is waiting, that client is unblocked and one or more CounterNotify events may be generated. If the change to the counter satisfies the trigger for an alarm, an AlarmNotify event is generated and the alarm is updated. An Access error is generated if counter is a system counter. A Counter error is generated if counter does not name a valid counter. If the resulting value for the counter would be outside the range for an INT64, a Value error is generated and the counter is not changed.

It should be noted that all the clients whose triggers are satisfied by this change are unblocked, so this request cannot be used to implement mutual exclusion.

SetCounter counter: COUNTER
value: INT64

Errors: Counter,Access

This request sets the value of the given counter to value.

The effect is equivalent to executing the appropriate

Synchronization Protocol

6 ChangeCounter request to change the counter value to value.

An Access error is generated if counter names a system counter. A Counter error is generated if counter does not name a valid counter.

CreateAlarm id: ALARM
values-mask: CARD32
values-list: LISTofVALUE
left">Errors: IDChoice,Counter,Match,Value,Alloc

This request creates an alarm and assigns the identifier id to it. The values-mask and values-list specify the attributes that are to be explicitly initialized. The attributes for an Alarm and their defaults are:

Attribute

Type

Default trigger

TRIGGER counter

None value-type

Absolute value

0test-type

PositiveComparison delta

INT64

1events

BOOL

TRUE

The trigger is initialized as described in the definition of

TRIGGER, with an error being generated if necessary.

If the counter is None, the state of the alarm is set to

Inactive, else it is set to Active.

Whenever the trigger becomes TRUE, either as a result of this request or as the result of a

SetCounter, ChangeCounter, DestroyCounter, or ChangeAlarm request, an AlarmNotify event is generated and the alarm is updated. The alarm is updated by repeatedly adding delta to the value of the trigger and reinitializing it until it becomes FALSE. If this update would cause value to fall outside the range for an INT64, or if the counter value is None, or if the delta is 0 and test-type is PositiveComparison or NegativeComparison, no change is made to value and the alarm state is changed to Inactive before the event is generated. No further events are generated by an Inactive alarm until a

ChangeAlarm or DestroyAlarm request is executed.

If the test-type is PositiveComparison or

PositiveTransition and delta is less than zero, or if the test-type is NegativeComparison or

NegativeTransition and delta is greater than zero, a

Match error is generated.

Synchronization Protocol

7 The events value enables or disables delivery of

AlarmNotify events to the requesting client. The alarm keeps a separate event flag for each client so that other clients may select to receive events from this alarm.

An AlarmNotify event is always generated at some time after the execution of a CreateAlarm request. This will happen immediately if the trigger is TRUE, or it will happen later when the trigger becomes TRUE or the Alarm is destroyed.

ChangeAlarm id: ALARM
values-mask: CARD32
values-list: LISTofVALUE

Errors: Alarm,Counter,Value,Match

This request changes the parameters of an Alarm. All of the parameters specified for the CreateAlarm request may be changed using this request. The trigger is reinitialized and an AlarmNotify event is generated if appropriate, as explained in the description of the CreateAlarm request.

Changes to the events flag affect the event delivery to the requesting client only and may be used by a client to select or deselect event delivery from an alarm created by another client.

The order in which attributes are verified and altered is server-dependent. If an error is generated, a subset of the attributes may have been altered.

DestroyAlarm alarm: ALARM

Errors: Alarm

This request destroys an alarm. An alarm is automatically destroyed when the creating client is closed down if the close-down mode is Destroy. When an alarm is destroyed, an AlarmNotify event is generated with a state value of

Destroyed.

QueryAlarm alarm: ALARM

=>
trigger: TRIGGER
delta: INT64
events: ALARMEVENTMASK
state: ALARMSTATE

Errors: Alarm

This request retrieves the current parameters for an Alarm.

SetPriority client-resource: XID

Synchronization Protocol

8 priority: INT32

Errors: Match

This request changes the scheduling priority of the client that created client-resource. If client-resource is None, then the priority for the client making the request is changed. A

Match error is generated if client-resource is not None and does not name an existing resource in the server. For any two priority values, A and B, A is higher priority if and only if

A is greater than B.

The priority of a client is set to 0 when the initial client connection is made.

The effect of different client priorities depends on the particular implementation of the extension, and in some cases it may have no effect at all. However, the intention is that higher priority clients will have their requests executed before those of lower priority clients.

For most animation applications, it is desirable that animation clients be given priority over nonrealtime clients.

This improves the smoothness of the animation on a loaded server. Because a server is free to implement very strict priorities, processing requests for the highest priority client to the exclusion of all others, it is important that a client that may potentially monopolize the whole server, such as an animation that produces continuous output as fast as it can with no rate control, is run at low rather than high priority.

GetPriority client-resource: XID

=>
priority: INT32

Errors: Match

This request returns the scheduling priority of the client that created client-resource. If client-resource is None, then the priority for the client making the request is returned. A

Match error is generated if client-resource is not None and does not name an existing resource in the server.

Events

CounterNotify counter: COUNTER
wait-value: INT64
counter-value: INT64
time: TIME
count: CARD16
destroyed: BOOL

CounterNotify events may be generated when a client becomes unblocked after an Await request has been processed. The wait-value is

Synchronization Protocol

9 the value being waited for, and counter-value is the actual value of the counter at the time the event was generated. The destroyed flag is TRUE if this request was generated as the result of the destruction of the counter and FALSE otherwise. The time is the server time at which the event was generated.

When a client is unblocked, all the CounterNotify events for the

Await request are generated contiguously. If count is 0, there are no more events to follow for this request. If count is n, there are at least n more events to follow.

AlarmNotify alarm: ALARM
counter-value: INT64
alarm-value: INT64
state: ALARMSTATE
time: TIME

AnAlarmNotifyeventisgeneratedwhenanalarmistriggered.alarmvalue is the test value of the trigger in the alarm when it was triggered, counter-value is the value of the counter that triggered the alarm, and time is the server time at which the event was generated. The state is the new state of the alarm. If state isInactive,nomoreeventswillbegenerated by this alarm until a ChangeAlarm request is executed, the alarm is destroyed, or the counter for the alarm is destroyed.

10 Chapter 2. Encoding

Please refer to the X11 Protocol Encoding document as this section uses syntactic conventions established there and references types defined there.

The name of this extension is "SYNC".

Encoding New Types

The following new types are used by the extension.

ALARM: CARD32

ALARMSTATE:

       0 Active

       1 Inactive

       2 Destroyed

COUNTER: CARD32

INT64: 64-bit signed integer

SYSTEMCOUNTER:

       4 COUNTER counter

       8 INT64 resolution

       2 n length of name in bytes

       n STRING8 name

       p pad,p=pad(n+2)

TESTTYPE:

       0 PositiveTransition

       1 NegativeTransition

       2 PositiveComparison

       3 NegativeComparison

TRIGGER:

       4 COUNTER counter

       4 VALUETYPE wait-type

       8 INT64 wait-value

       4 TESTTYPE test-type VALUETYPE:

       0 Absolute

       1 Relative

WAITCONDITION:

       20 TRIGGER trigger

       8 INT64 event threshold

An INT64 is encoded in 8 bytes with the most significant 4 bytes first followed by the least significant 4 bytes. Within these 4-byte groups, the byte ordering determined during connection setup is used.

Encoding Errors

Counter

        1 0 Error

        1 Base + 0 code

        2 CARD16 sequence number

        4 CARD32 bad counter

        2 CARD16 minor opcode

Encoding

11 1 CARD8 major opcode

        21 unused

Alarm

        1 0 Error

        1 Base + 1 code

        2 CARD16 sequence number

        4 CARD32 bad alarm

        2 CARD16 minor opcode

        1 CARD8 major opcode

        21 unused

Encoding Requests

Initialize

        1 CARD8 major opcode

        1 0 minor opcode

        2 2 request length

        1 CARD8 major version

        1 CARD8 minor version

        2 unused

=>

        1 1 Reply

        1 unused

        2 CARD16 sequence number

        4 0 reply length

        1 CARD8 major version

        1 CARD8 minor version

        2 unused

        20 unused

ListSystemCounters

        1 CARD8 major opcode

        1 1 minor opcode

        2 1 request length

=>

        1 1 Reply

        1 unused

        2 CARD16 sequence number

        4 0 reply length

        4 INT32 list length

        20 unused

        4n list of SYSTEMCOUNTER system counters

CreateCounter

        1 CARD8 major opcode

        1 2 minor opcode

        2 4 request length

        4 COUNTER id

        8 INT64 initial value

DestroyCounter

        1 CARD8 major opcode

Encoding

12 1 6 minor opcode_1

        2 2 request length

        4 COUNTER counter

=>

        1 1 Reply

        1 unused

        2 CARD16 sequence number

        4 0 reply length

        8 INT64 counter value

        16 unused

Await

        1 CARD8 major opcode

        1 7 minor opcode_2

        2 1 + 7*n request length

        28n LISTofWAITCONDITION wait conditions

ChangeCounter

        1 CARD8 major opcode

        1 4 minor opcode_3

        2 4 request length

        4 COUNTER counter

        8 INT64 amount

SetCounter

        1 CARD8 major opcode

        1 3 minor opcode_4

        2 4 request length

        4 COUNTER counter

        8 INT64 value

CreateAlarm

        1 CARD8 major opcode

        1 8 minor opcode

        2 3+n request length

        4 ALARM id

        4 BITMASK values mask

             #x00000001 counter

             #x00000002 value-type

             #x00000004 value

             #x00000008 test-type

             #x00000010 delta

             #x00000020 events

        4n LISTofVALUE values

VALUES

        4 COUNTER counter

1A previous version of this document gave an incorrect minor opcode

2A previous version of this document gave an incorrect minor opcode.

3A previous version of this document gave an incorrect minor opcode.

4A previous version of this document gave an incorrect minor opcode.

Encoding

13 4 VALUETYPE value-type

        8 INT64 value

        4 TESTTYPE test-type

        8 INT64 delta

        4 BOOL events

ChangeAlarm

        1 CARD8 major opcode

        1 9 minor opcode

        2 3+n request length

        4 ALARM id

        4 BITMASK values mask

             encodings as for CreateAlarm

        4n LISTofVALUE values

             encodings as for CreateAlarm

DestroyAlarm

        1 CARD8 major opcode

        1 11 minor opcode_5

        2 2 request length

        4 ALARM alarm

QueryAlarm

        1 CARD8 major opcode

        1 10 minor opcode_6

        2 2 request length

        4 ALARM alarm

=>

        1 1 Reply

        1 unused

        2 CARD16 sequence number

        4 2 reply length

        20 TRIGGER trigger

        8 INT64 delta

        1 BOOL events

        1 ALARMSTATE state

        2 unused

SetPriority

        1 CARD8 major opcode

        1 12 minor opcode

        2 3 request length

        4 CARD32 id

        4 INT32 priority

GetPriority

        1 CARD8 major opcode

        1 13 minor opcode

        2 1 request length

        4 CARD32 id

=>

5A previous version of this document gave an incorrect minor opcode.

6A previous version of this document gave an incorrect minor opcode.

Encoding

14 1 1 Reply

1 unused

2 CARD16 sequence number

4 0 reply length

4 INT32 priority

20 unused

Encoding Events

CounterNotify

        1 Base + 0 code

        1 0 kind

        2 CARD16 sequence number

        4 COUNTER counter

        8 INT64 wait value

        8 INT64 counter value

        4 TIME timestamp

        2 CARD16 count

        1 BOOL destroyed

        1 unused

AlarmNotify

        1 Base + 1 code

        1 1 kind

        2 CARD16 sequence number

        4 ALARM alarm

        8 INT64 counter value

        8 INT64 alarm value

        4 TIME timestamp

        1 ALARMSTATE state

        3 unused